# [](https://github.com/climateguard/RadSens#official-library-for-radsens-by-climateguard)Official RadSens library by ClimateGuard

**RadSens is an unique ultracompact I2C-connectable dosimeter module based on a Geiger tube.**

**Advantages:**
- Low cost of a module  
- Super-easy to use  
- High compatibility with all devices  
- Small dimensions (from 88x21 mm to 120x21 mm)  
- Universatility in use (you can mount any Geiger tube, it is provided that the board can be shortened for a shorter tube)  
- The measurement accuracy is limited only by the sensitivity of the tube, which can be changed programmatically for recalculation

Learn more about features of CG-Anem in [extras](https://github.com/climateguard/RadSens/tree/master/extras)

**You can buy RadSens at:**

-  [Tindie](https://www.tindie.com/stores/climateguard/)  
-  [Aliexpress](https://aliexpress.ru/store/all-wholesale-products/910985005.html)  
-  [Alibaba](https://mashintertorg.trustpass.alibaba.com/productgrouplist-903279422/Electronics.html?spm=a2700.shop_cp.88.14)

## Installation
**For Arduino IDE:**
- You can download .zip file of  library from GitHub or add it by Arduino Library Manager ("Arduino IDE -> Sketch -> Include library -> Manage libraries..." or by Ctrl+Shift+I shortcut) by mentioning "RadSens" in the search bar.

**For other IDEs:**

- Download .zip file and unpack it to the libraries folder of your project.


## [](https://github.com/climateguard/RadSens#instructions)Instructions

You can find datasheet and example connection schemes in  ["extras" folder](https://github.com/climateguard/RadSens/tree/master/extras/)  
Also you can check video guides in our [YouTube Channel](https://www.youtube.com/channel/UCp0ztK0nSK1sWZI-IgQqJeQ)

## [](https://github.com/climateguard/RadSens#instructions-for-esphome-and-home-assistant)Instructions for ESPHome and Home Assistant

[Instructions for connecting RadSens to ESPHome by @maaad](https://github.com/maaad/RadSens1v2)

Thanks author @maaad for instruction and code!

**To run device in ESPhome you need to add folder "RadSens1v2" to your ESPHome directory and follow the instruction above to add Radsens to device config.**

## [](https://github.com/climateguard/RadSens#contact-us)Contact us
- [ClimateGuard Community in Telegram](https://t.me/climateguard_community)  
- [Our YouTube channel](https://www.youtube.com/channel/UCp0ztK0nSK1sWZI-IgQqJeQ)
